# Steps:

1. step:start
2. Step:add libraries
3. Step:Define SSID&Password
4. Step:Give IP Static from the same network
5. Step:Give Subnet &IP Getway
6. Step:connect to the network
7. Step:check wi-fi is connected to wi-fi network No print(check wi-fi is connected to wi-fi network) Yes print(WiFi connected…!)
8. Print local IP